Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Testing the Digital Networking and TCP/IP Connection > Correcting Diagnostic Failures
| Correcting Diagnostic Failures
To correct diagnostic failures for the Avaya INTUITY system: On the Test Packet results page, click Cancel. The system displays the Send & Receive Test Packets From page. Verify that the IP address you entered into the IP Address: field is correct: If it does not match, re-enter the correct address and repeat the Transmitting Test Packets procedure. If it matches, continue with Step 3. Click Cancel until you reach the TCP/IP Administration and Diagnostics page. Complete the procedure Establishing Network Addresses. Continue with Attaching the LAN Cable. Return to this procedure after you have attached the LAN cable and attempt the test again. If the test is successful, continue with Verifying the IP Address for Remote Machines. If the test fails a second time, contact your remote support center. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.