#### Audio Push Message (PM)

The first step in sending an Audio push is to send an HTTP POST request from the Push Initiator to the telephone’s Push Agent. Following is the XML Message (PM) format sent from the Push Initiator to the Push Agent:

    <?xml version="1.0"?>

    <Push

    	alert=“0|1|2|3”

    	type=“audio”

    	mode=“normal|barge”

    >

       <go href=“http://trusted_push_server/filename.xml”   method=“get|post”>

    	<postfield name=“name1” value=“value1”/>

    	<postfield name=“name2” value=“value2”/>

    </go>

    </Push>