### Syntax Implementation

#### Click to Dial Functionality

To enable the click to dial functionality, use the following syntax:

wtai://wp/mc;number

You can embed this code into any valid WML tag that implements href or a hyperlink by associating these tags with a <go> tag. Examples of tags you can associate with the <go> tag are the <a> tag, <anchor>, <do>, <option>, or <onevent> tags.

##### Click-to-dial using <a> tag:

    	<?xml version=”1.0”?>

    	<!DOCTYPE wml PUBLIC “-//WAPFORUM//DTD WML 1.3//EN”

                 “http://www.wapforum.org/DTD/wml13.dtd”>

    		<wml>

    		<card id=”callid1” title=”Click-to-Dial Demo”>

    			<p>

    				Click on the link to originate a call

    				<a href=”wtai://wp/mc;5551212”>Call 5551212</a>

    			</p>

    	</card>

    </wml>

The generated code is rendered as the following diagram:

The code shows a hyperlink as Call 5551212 on the Web screen of an Avaya 9620 IP Telephone. A phone icon precedes this hyperlink, indicating the hyperlink is a “click-to-dial” number. When a user selects this link, the phone dials the string “5551212” or any phone number that follows a semicolon in the WTAI code.

NOTE: A phone icon is generated only when an <a> tag or <anchor> tag is used.

##### Click-to-dial using <anchor> tag:

    <?xml version=”1.0”?>

    <!DOCTYPE wml PUBLIC “-//WAPFORUM//DTD WML 1.3//EN”

                 “http://www.wapforum.org/DTD/wml13.dtd”>

    <wml>

    		<card id=”callid1” title=”Using anchor tag”>

    			<p>

    				<p align=”center”>***Customer Service***</p>

    			</p>

    				Your order will ship in 3-5 days.

    				If you have any questions, then

    				<anchor>Call us

    					<go href=”wtai://wp/mc;5551212”/>

    				</anchor>

    			</p>

    	</card>

    </wml>

The generated code is rendered as the following diagram:

The code shows a hyperlink as Call Us on the Web page. When a user selects this link, the phone dials the string “5551212” or any number that follows a semicolon in the WTAI code.

##### Click-to-dial using <onevent> tag:

    <?xml version=”1.0”?>

    <!DOCTYPE wml PUBLIC “-//WAPFORUM//DTD WML 1.3//EN”

                 “http://www.wapforum.org/DTD/wml13.dtd”>

    <wml>

    	<card id=”callid3” title=”Incorrect Login”>

    		<onevent type=”ontimer”>

    						<go href=”wtai://wp/mc;+ 1888 555 1212"/>

    			</onevent>

    		<timer value="50"/>

    		<p>

    You have exceeded number of tries.

    				A call will be automatically launched in 5 seconds.

    		</p>

    </card>

    </wml>

The generated code is rendered as the following diagram:

The code automatically dials the number “1 888 555 1212" after 5 seconds, once the Web page loads.

NOTE: When using international numbers with click to dial functionality, you must include a '+' before the country code. You must include a space following the country code, but before the national number. The enhanced local dialing rules will then be handled correctly. See the Avaya one-X Deskphone Edition for 9600 Series IP Telephone Administrator Guide for configuration information.

##### Click-to-dial using <do> tag (softkey):

    <?xml version=”1.0”?>

    <!DOCTYPE wml PUBLIC “-//WAPFORUM//DTD WML 1.3//EN”

                 “http://www.wapforum.org/DTD/wml13.dtd”>

    <wml>

    		<card id=”callid4” title=”Click-to-Dial Demo”>

    			<p>

    				Contact us for more information.

    			</p>

    			<do type=”accept” label=”Call Us” name=”dotag1”>

    				<go href=”wtai://wp/mc;+1 8005552525”/>

    			</do>

    	</card>

    </wml>

The generated code is rendered as the following diagram: