## Local Administrative Options Using the Telephone Dialpad

The Avaya one-X Deskphone Edition for 9600 IP Telephones Installation and Maintenance Guide details how to use local procedures at the telephone for administration. The local procedures you use most often as an administrator are:

- CLEAR - Remove all administered values, user-specified data, option settings, etc. and return a telephone to its initial “out of the box” default values.
- DEBUG - Enable or disable debug mode for the button module serial port.
- GROUP - Set the group identifier on a per-phone basis.
- RESET - Reset the telephone to default values including the registration extension and password, any values administered through local procedures, and values previously downloaded using DHCP or a settings file.
- RESTART - Restart the telephone in response to an error condition, including the option to reset system values.
- VIEW - Review the 9600 IP Telephone system parameters to verify current values and file versions.
- Secondary Ethernet (Hub) Interface Enable/Disable - Enable or disable the secondary Ethernet hub locally.