#### Editing Custom Options

Use the following procedure to edit custom options.

1. Highlight the newly created scope.
2. Select DHCP Options-->Defaults in the menu.
3. Click the New button.
4. In the Add Option Type dialog box, enter an appropriate custom option name, for example, “9600OPTION.”
5. Change the Data Type Byte value to String.
6. Enter 242 in the Identifier field.
7. Click the OK button.

The DHCP Options menu displays.

1. Select the Option Name for 242 and set the value string.
2. Click the OK button.
3. For the Option Name field, select 003 Router from the drop-down list.
4. Click Edit Array.
5. Enter the Gateway IP Address recorded in Table 3: Required Network Information Before Installation - Per DHCP Server for the New IP Address field.
6. Select Add and then OK.