### Aliasing 9600 Series IP Telephones

On Communication Manager releases earlier than 4.0, which do not provide native support for 96xx IP Telephones, administer (alias) the 9620 IP Telephone as a 4610 IP Telephone and the administer the 9630 IP Telephone as a 4620/4621 IP Telephone.

Change Alias Station:

- Alias set up type 9620 to a 4610
- Alias set up type 9630 to a 4620

The 9620 IP Telephone supports twelve administrable telephony call appearances or features. As such, assign only the first twelve of the twenty four buttons on the 4610 Station form. The 9620 IP Telephone does not support the SBM24 Button Module.

The 9630 IP Telephone supports twenty four administrable telephony call appearances or features. In addition, the 9630 IP Telephone supports the SBM24 Button Module.

The SBM 24 Button Module provides another twenty four administrable call appearances and features. The button module can be used freestanding or attached directly to the 9630.