#### Barge Priority

When the mode attribute in the <Push> tag is set to barge, the Top Line Push Content is accepted as a priority message. However, a barge Top Line push is rejected when the telephone is in one of these non-pushable states:

- When the telephone is in the process of restoring a retrieved backup file, or
- When a Local Procedure has been initiated. See the Avaya one-X Deskphone Edition for 9600 Series IP Telephones Administrator Guide on the Avaya support Web site for more details on Local maintenance procedures.

In either non-pushable state, the barge content, including any notification tones, is discarded. In all other cases, the telephone must accept the barge request and display the barge Top Line message immediately.