### Configuring the General Directory Application Administration Screen

To configure the General Directory Application Administration screen:

1. From the Welcome screen, select the General Administration screen link. Alternately, select the Right Arrow icon at the bottom of the Welcome screen.

Figure 33: Directory Application Administration Screen

1. All fields except Directory User ID and Directory Password are required. Table 13 shows the Administration screen fields, their associated key names, default values, and descriptions:

Table 13: Administration Screen Fields
Field Title | Key Name | Default | Description
--- | --- | --- | ---
Application Title | DIRSVRNAME | 4620 Directory Application | Label appearing at top of the user interface’s Directory Search screen.
Directory Server | DIRSRVR | Null | LDAP server address, IP address or fully qualified DNS name.
Topmost Distinguished Name (Search Root) | DIRTOPDN | Null | The search root base, usually “ou=people” or o=company name. Note that spaces and other special characters might need to be treated as specified in RFC 2253, Lightweight Directory Access Protocol (v3): UTF-8 String Representation of Distinguished Names.
Port Network | DIRLDAPPORT | 389 for LDAP 686 for SSI-enabled LDAP | Directory Server Port.
Max number of hits |  | 96 | The maximum number of result entries that can be displayed on the 4620.
Directory User ID | DIRUSERID | Optional | User name for authorized Directory search, if required.
Directory Password | DIRSRVRPWD | Optional | User’s password for authorized Directory search, if required.
Directory Search Time | DIRSEARCHTIME | 10 seconds | Maximum amount of time the application waits for search results (01 - 59 seconds).
Directory Coding | DIRCODING | Latin 1 | No other option is currently available.

1. Press the Save Changes button as stated at the bottom of the screen to save the values entered. When you complete the final administration screen, you can review all values on all screens.