Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Testing the Digital Networking and TCP/IP Connection > Receiving Voice Messages from Remote Test Subscribers
| Receiving Voice Messages from Remote Test Subscribers
Have remote test subscribers send messages to your local test subscribers during acceptance testing. You need to retrieve the messages to verify that your local machine is administered correctly with the remote machines and is receiving messages correctly. When you retrieve the messages, you should hear the system say the name of the remote machine and the remote test subscriber, if you recorded a name for the remote machine and the remote test subscriber. After you receive messages from the remote machines, contact each of the remote machine network administrators and inform each one that you received a message from their machine. To retrieve messages from the test remote subscribers: Dial the INTUITY AUDIX voice messaging extension. This is the extension subscribers call to retrieve and send messages. When prompted to enter an extension, use the telephone keypad to enter a local test subscriber extension followed by #. Enter the password for the local test subscriber followed by #. You hear the subscriber's name and a message telling you the number of messages in your mailbox, if any. Avaya INTUITY then plays the activity menu. Press 2 to retrieve messages. Avaya INTUITY plays the header for the first message. The header includes the name or extension of the sender and the date and time the message was received. Press 0 to listen to the message. As you listen to the message, note the remote machines and remote test subscribers that were able to exchange messages with you. At the end of the message, you hear the following prompt: `"To respond or forward, press one. To delete, press star d. To skip, press pound."` Press * 3 (which is the same as * D) to delete the message. Repeat Step 4 through Step 7 for each message in the local test subscriber's mailbox. When you finish retrieving messages from remote test subscribers, hang up the telephone and then contact the remote machine network administrators and inform them that you received a message from their machine. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.