Search This CD Index Contact Us
Home > Administration > Reports > Remote Messages Monthly Traffic Screen
| Remote Messages Monthly Traffic Screen
> Table: Field Definitions: Remote Messages Monthly Screen
> Field Name | Description/Procedure
> --- | ---
> Machine Name: | The name of the remote machine you entered on the command line.
> Machine Type: | The type of remote machine, for example, calld or AUDIX.
> Date: | The starting month for which traffic data was collected for the report. It is the month you entered on the command line or the current date if you did not specify a month. If you enter a month previous to the current month, each month's record is presented as an additional page (screen). Press F7 (NextPage) and F8 (PrevPage) to scroll through each monthly report record.
> Ending Date: | The day on which data collection ended.
> LOCAL ORIGINATION
> Prime/Non-Prime | Whether message transmission came from the local AUDIX during a period specified as prime or nonprime time.
> Transfer Sessions: | The number of message transfer sessions that occurred during the reporting period. For AMIS analog messages, each transmission or reception session is pegged as a transfer session.
> Usage (seconds): | The total number of seconds for all message transfer sessions that occurred during the reporting period. AMIS analog messages are included in this total.
> Average Usage: | The average length, in seconds, of a message transfer session. AMIS analog messages are included in this total.
> Messages Sent: | The total number of messages sent from the local AUDIX machine to the remote AUDIX machine. AMIS analog messages are included in this total.
> Voice Components: | The total number of voice components sent from the local AUDIX machine to the remote AUDIX machine. AMIS analog messages are included in this total.
> FAX Components: | The total number of fax components sent from the local AUDIX machine to the remote AUDIX machine. Call delivery messages are included in this total.
> Binary Attachments: | The total number of binary attachments sent from the local AUDIX machine to the remote AUDIX machine.
> Text Components: | The total number of text components sent from the local AUDIX machine to the remote AUDIX machine.
> Messages Rejected: | The total number of messages rejected by the local AUDIX machines during the reporting period. AMIS analog messages are included in this total. For call delivery machines, if there is no positive confirmation, the message is recorded as rejected.
> Status Sent: | The total number of status reports sent by the local AUDIX machine to the remote AUDIX machine for messages originated by the remote AUDIX machine. This number is 0 for call delivery machines.
> Status Received: | Not applicable.
> Admin Updates: | The total number of administration updates (name, voice name, extension, community changes, add and delete local subscribers) sent from the local AUDIX machine to the remote AUDIX machine. This field applies to digital network machines only.
> REMOTE ORIGINATION
> Prime/Non-Prime | Whether message transmission came from the remote AUDIX during a period specified as prime or nonprime time.
> Transfer Sessions: | The number of message transfer sessions that occurred during the reporting period. For AMIS analog messages, each transmission or reception session is pegged as a transfer session.
> Usage (seconds): | The total number of seconds for all message transfer sessions that occurred during the reporting period. AMIS analog messages are included in this total.
> Average Usage: | The average length, in seconds, of a message transfer session. AMIS analog messages are included in this total.
> Messages Sent: | The total number of messages sent from the remote AUDIX machine and received by the local AUDIX machine during the reporting period. AMIS analog messages are included in this total.
> Voice Components: | The total number of voice components sent from the remote AUDIX machine and received by the local AUDIX machine during the reporting period. AMIS analog messages are included in this total.
> FAX Components: | The total number of voice components sent from the remote AUDIX machine and received by the local AUDIX machine during the reporting period. Call delivery messages are included in this total.
> Binary Attachments: | The total number of binary attachments sent from the remote AUDIX machine and received by the local AUDIX machine during the reporting period.
> Text Components: | The total number of text components sent from the remote AUDIX machine and received by the local AUDIX machine during the reporting period.
> Messages Rejected: | The total number of messages rejected by the local and remote AUDIX machines during the reporting period. AMIS analog messages are included in this number. For call delivery machines, if there is no positive confirmation, the message is recorded as rejected.
> Status Sent: | Not applicable.
> Status Received: | The total number of status reports received by the local AUDIX machine for messages that the local machine sent to the remote AUDIX machine. This field is not applicable for AMIS analog messages.
> Admin Updates: | The total number of administration updates (name, voice name, extension, community changes, add and delete local subscribers) sent from the remote AUDIX machine to the local AUDIX machine. This field applies to digital network machines only.
> Message Transmission Threshold Exceptions: | The number of times the local node exceeded its message transmission threshold. This field is not applicable for AMIS analog machines.
> Session Failures Far End "No Answer": | The number of unsuccessful call attempts from the local AUDIX machine to the remote AUDIX machine. AMIS analog session failures are included in this count.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.