Search This CD Index Contact Us
Home > Administration > Networking > AMIS Analog Networking > AMIS Analog Networking Administration > Adjusting the System Limits
| Adjusting the System Limits
> 2. You might have to adjust the system limits to accommodate additional administered remote subscribers and/or message delivery recipients for either the AMIS Analog Networking or Message Delivery features. Only remote subscribers on systems administered for AMIS one-step addressing or Message Delivery recipients can be administered on the local system. To adjust the system limits to accommodate administered remote subscribers: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. At the `enter command:` prompt, enter list measurements feature day. The system displays the Feature Daily Traffic screen. Record the number displayed in the `Local:` field for use later with the System Parameters Limits screen.
>    Note: Consider adding the number of local subscribers that the system administrator expects to administer over the next 12 months to the number shown on the screen.
Record the number of subscribers displayed in the `Remote:` and `Non Administered Remote:` fields for use later with the System Parameters Limits screen. Press F3 (Cancel). The system displays the AUDIX Command Prompt screen. At the `enter command:` prompt, enter change system-parameters limits. The system displays the System-Parameters Limits screen. Enter the number of local subscribers in the `Subscribers, Local:` field. Enter the number of remote subscribers you expect to administer on the local system in the`Administered Remote:` field. Press F3 (Enter). Continue with Administering Retransmission Intervals. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.