Search This CD Index Contact Us
Home > Maintenance > Getting Inside the Platform > Removing Power From the Platform
| Removing Power From the Platform
The platform requires a dedicated circuit with a dedicated circuit breaker. The power cord connects to the rear of the system to the AC power inlet receptacle. See Back View of Platform. Before you open the PC, you must remove power to the system. To remove power: Shut down the system. Turn off the monitor's power button. Verify that the monitor's power is off. Turn off the power by pressing the power button on the front of the chassis. See Front View of Platform. The green power lamp on the front of the unit should be off. Unplug the power cord from the AC receptacle in the wall. If necessary, unplug the monitor cord from the PC. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.