Search This CD Index Contact Us
Home > Administration > Reports > Feature Daily Traffic Screen, Page 1
| Feature Daily Traffic Screen, Page 1
> Table: Field Definitions: Feature Daily Traffic Screen, Page 1
> Field Name | Description/Procedure
> --- | ---
> Date: | The starting date for which traffic data was collected for the report. It is the date you entered on the command line or the current date if you did not specify a date. If you enter a date previous to the current date, each day's record is presented as an additional page (screen). Press F7 (NextPage) and F8 (PrevPage) to scroll through each daily report record.
> Ending Time: | The time at which data collecting ended.
> Maximum Average Voice Ports in Use: | The average number of ports that were in use simultaneously during the busiest hour of the day you selected. See Interpreting Traffic Report Findings to analyze this information.
> Maximum Average IMAPI Sessions in Use: | The average number of IMAPI sessions that were in use simultaneously during the busiest hour of the day you selected. See Interpreting Traffic Report Findings to analyze this information.
> SUBSCRIBERS
> Local: | The total number of local subscribers administered on the AUDIX system at the end of the day being reported.
> Remote: | The total number of remote subscribers administered on the AUDIX system at the end of the day being reported.
> Non Administered Remote: | The total number of subscribers external to the AUDIX system (not administered) who sent mail to an administered AUDIX subscriber or to whom mail was sent by an administered AUDIX subscriber at the end of the day being reported.
> VOICE MAIL
> Successful Logins, External: Successful Logins, Internal: Successful Logins, Client Logins: | The number of successful login attempts made during the day reported. Login attempts were made by subscribers calling from: Telephones not administered (external) on the host switch Telephones administered (internal) on the host switch IMAPI interface (client logins)
> Failed Logins, External: Failed Logins, Internal: Failed Logins, Client Logins: | The number of unsuccessful login attempts made during the day reported. Login attempts were made by subscribers calling from: Telephones not administered (external) on the host switch Telephones administered (internal) on the host switch IMAPI interface (client logins) Unsuccessful means that the AUDIX system did not allow the caller access to AUDIX operations. Denial to access could have been due to an unrecognizable password, login ID, or both, or because the caller hung up before completing the call.
> Session Usage (Seconds): | The total number of seconds that AUDIX ports were in use for voice mail sessions during the day reported.
> Session Usage: | The total number of seconds that IMAPI sessions were in use for voice mail sessions during the day reported.
> CALL ANSWER
> Completed Calls, External: Completed Calls, Internal: Completed Calls, Network: | The number of completed call answer telephone calls made to the AUDIX system during the day reported. Calls came from: Telephones not administered (external) on the host switch Telephones administered (internal) on the host switch Telephones networked with IMAPI sessions to the host switch These numbers include the times the AUDIX system answered calls for subscribers, attendants, and bulletin boards.
> Voice Components, External: Voice Components, Internal: Voice Components, Network: | The number of voice components that were included in call answer telephone calls made to the AUDIX system during the day reported. Calls came from: Telephones not administered (external) on the host switch Telephones administered (internal) on the host switch Telephones networked with IMAPI sessions to the host switch These numbers include the times the AUDIX system answered calls for subscribers, attendants, and bulletin boards.
> FAX Components, External: FAX Components, Internal: FAX Components, Network: | The number of fax components that were included in call answer telephone calls made to the AUDIX system during the day reported. Calls came from: Telephones not administered (external) on the host switch Telephones administered (internal) on the host switch Telephones networked with IMAPI sessions to the host switch These numbers include the times the AUDIX system answered calls for subscribers, attendants, and bulletin boards.
> Abandoned Calls, External: Abandoned Calls, Internal: Abandoned Calls, Network: | The number of times a caller hung up after the mailbox greeting started to play, but before the beep, to leave a message. Calls came from: Telephones not administered (external) on the host switch Telephones administered (internal) on the host switch Telephones networked with IMAPI sessions to the host switch These numbers include the times the AUDIX system answered calls for subscribers, attendants, and bulletin boards.
> Session Usage (seconds): | The total number of seconds that AUDIX ports were used for call answer sessions during the day being reported.
> Session Usage: | The total number of seconds that IMAPI sessions were used for call answer sessions during the day being reported.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.