Search This CD Index Contact Us
Home > Maintenance > Events > SM (Station Manager) Events
| SM (Station Manager) Events
The following events are generated by the SM application and indicate a problem with the station manager:
SM101 SM102 SM103 SM104 SM105 |  | SM106 SM107 SM108 SM201 |  |
### SM SM101 ##### Description: The INTUITY AUDIX LX system cannot get certain application information. ##### Repair Procedure: Contact your remote support center. ### SM SM102 ##### Description: The application code is too large. ##### Repair Procedure: Contact your remote support center. ### SM SM103 ##### Description: The system could not find the switch ID. ##### Repair Procedure: Contact your remote support center. ### SM SM104 ##### Description: The system received a script message from the wrong channel or mode. ##### Repair Procedure: No corrective action is necessary. ### SM SM105 ##### Description: The system is reporting that no switch is active. ##### Repair Procedure: Contact your remote support center. ### SM SM106 ##### Description: The switch link is down. ##### Repair Procedure: Contact your remote support center. ### SM SM107 ##### Description: A timeout occurred. A switch audit on the switch side can cause this condition. ##### Repair Procedure: If the system issues this message frequently, contact your remote support center. ### SM SM108 ##### Description: A message-waiting lamp (MWL) update failed for a subscriber. The MWL is an indicator that alerts subscribers that they have received new mail messages. ##### Repair Procedure: Contact your remote support center. ### SM SM201 ##### Description: The system failed to locate the indicated user. ##### Repair Procedure: Update the subscriber information. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.