Search This CD Index Contact Us
Home > Maintenance > TCP/IP Diagnostics > Viewing LAN Packet Statistics > View Packet Statistics - TCP/IP Diagnostics Page (Routing Statistics Option)
| View Packet Statistics - TCP/IP Diagnostics Page (Routing Statistics Option)
> Table: Field Definitions: Routing Statistics
> Column | Description
> --- | ---
> Destination | The destination network or host.
> Gateway | The gateway address.
> Genmask | The netmask for the destination network.
> Flags | The possible flags are: U: Route is up H: Target is a host G: Use gateway R: Reinstate route for dynamic routing D: Dynamically installed by daemon or redirect M: Modified from routing daemon or redirect A: Installed by addrconf C: Cache entry I: Reject route
> MSS | The maximum segment size for the TCP connections over this route.
> Window | The default window size for TCP connections over this route.
> irtt | The initial RTT (round trip time).
> iface | The interface to which packets for this route will be sent.
### ### ### ### Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.