Search This CD Index Contact Us
Home > Getting Started > Installation > Add Switch Integration Software and Language Packages
| Add Switch Integration Software and Language Packages
> > You need configuration notes or a switch integration worksheet to perform the steps in this section. This section includes steps for the following processes: Install additional language software Install switch integration software Select the switch integration ## Install Additional Language Software The language packages, also called announcement sets, allow system users to hear voice prompts and system announcements in other languages. The system is shipped from the factory with the following language packages installed: US English English TDD (for teletype (TTY) machines) To install additional announcement sets: Log on as craft (for a new installation) or sa (if restoring a system). The sa default password is sapasswd. From the Messaging Administration main menu, select:
> >     Software Installation
> > Follow the on-screen instructions to insert the DVD. Click DVD (or another installation media if applicable). The system warns you that system data should be backed up. If necessary perform a system backup. If the system is new, no data needs to be backed up. Click Continue Operation. The system displays a list of packages available on the DVD, either software packages or additional language sets depending on which DVD you have inserted. Packages that have already been installed are marked with "=". Select the language packages you want to install. Press PageDown to see the bottom of the page, then click Install selected packages. The system displays a list of packages to be installed. Review the list, then click Proceed with installation. The system begins the installation and displays installation status messages. The installation is complete when the pointer changes from a wristwatch to an X. After the software is installed, press PageDown to see the bottom of the status page. If all software was installed successfully, remove the DVD from the DVD drive. Click Restart the System. After the system restarts, press Enter to return to the prompt, and log in. From the Messaging Administration main menu, select:
> >     Start Messaging
> If the system is to be shipped, stop the voice system and power off the system. If the system is to be administered now, go to Install Switch Integration Software. ## Install Switch Integration Software
> NOTE: Before continuing, confirm that the switch integration you plan is generally available (GA). For more information about the GA integrations or to submit your integration for Controlled Introduction testing, see Switch Integration.
> > Install one of the two switch integration packages. The system default is that no switch integration package is installed. The two choices are: LANset SWINset You can only have one switch integration software package installed on the system at one time. If one package is already installed and you want another, you must remove the first package before installing the second package. Log on as craft (for a new installation) or sa (if restoring a system). The sa default password is sapasswd. From the Messaging Administration main menu, select:
> >     Software Installation
Switch Integration software is included on the main INTUITY AUDIX LX software DVD. Obtain the DVD, then follow the on-screen instructions to insert the DVD. Click DVD (or another installation media if applicable). The system warns you that system data should be backed up. If necessary, perform a system backup. If the system is new, no data needs to be backed up. The system displays a list of packages available on the DVD, including the two switch integration packages: LANset and SWINset. Select the switch integration package you want to install. If you know which type of switch integration you plan to do, based on configuration notes, select the corresponding software package. You can only have one switch integration software package installed on the system at one time. Press PageDown to see the bottom of the page, and click Install selected packages. The system displays a list of packages to be installed. Review the list, then click Proceed with installation. The system begins the installation and displays installation status messages. The installation is complete when the pointer changes from a wristwatch to an X. After the software is installed, press PageDown to see the bottom of the status page. If the software was installed successfully, remove the DVD from the DVD drive. Click Restart the System. After the system restarts, it displays the message: Press Enter to return to prompt... Press Enter, then log in. If the system is to be moved or shipped, stop the voice system and power off the system. If system data is to be restored, go to Performing a Restore. If the system is to be administered now, go to the next section. ## Select the Switch Integration When the appropriate switch integration software package is installed, select the switch integration type: From the Messaging Administration main menu, select: Switch Selection The system displays the Switch Selection page with a drop-down list of switch configurations. The list varies depending on which switch software package you installed. Click on the drop-down list and select the switch and country that matches the customer site. Click Save. The system displays a confirmation message and also a message that says you need to stop and start the Voice System. Stop and start the Voice System. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.