Search This CD Index Contact Us
Home > Administration > Networking > AMIS Analog Networking > AMIS Analog Networking Administration > Activating the AMIS Feature Parameter Changes
| Activating the AMIS Feature Parameter Changes
You must run the following audits on the local system to activate the AMIS Analog Networking feature parameters: Network-Data Audit Subscriber-Data Audit ### Network-Data Audit To run an audit and activate changes: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. At the `enter command:` prompt, type audit network-data. The system displays the Audit Results screen. Press F3 (Enter) to execute the audit. The system runs the audit. When the audit is complete, the system displays the outcome of the audit in the Results column, the cursor returns to the command line, and the system displays the following message: `Command Successfully Completed`. ### Subscriber-Data Audit To run an audit and activate any changes made to the System-Parameters Features screen: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. At the `enter command:` prompt, type audit subscriber-data. The system displays the Audit Results screen. Press F3 (Enter) to execute. The system runs the audit. When the audit is complete, the system displays the outcome of the audit in the Results column, the cursor returns to the command line, and the system displays the following message: `Command Successfully Completed`. ### ### ### Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.